{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":11,"n_cols":6,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[null,"1.)","Number of Bolt ROWS","    =",3]
[null,"2.)","Number of BOLT COLUMNS","    =",2]
[null,"3.)","Spacing of ROWS","    =",3,"in"]
[null,"4.)","Spacing of COLUMNS","    =",3,"in"]
[null,"5.)","Eccentricity","    =",6,"in"]
[null,"6.)","Rotation","    =",0,"deg"]
[]
[null,"7.)","Coefficent,  C","    =",{"$f":"BoltCoefficient(E4,E5,E6,E7,E8,E9)","v":2.2515377819595153}]